|  |  |
| --- | --- |
| FT: | **08 33 23** |
| **ITEM:** | **Overhead Coiling Doors** |
| **DOOR TYPE:** |  |
| **AREA SERVED:** |  |

Form Filled Out By:

|  |  |  |
| --- | --- | --- |
|  | **Name & Company** | **Date** |
| GC |  |  |
| PC |  |  |
| EC |  |  |
| BC |  |  |
| CC |  |  |
| OR |  |  |
| A/E |  |  |
| CA |  |  |

GC = General Contractor; PC = Plumbing Contractor; EC = Electrical Contractor; BC = Balancing Contractor; CC = Controls Contractor; OR = Owner Representative; A/E = Architect/Engineer; CA = Commissioning Agent

XX = No Initials Required

# TEST PREREQUISITES

The following items have been completed and the equipment is ready for Functional Testing.

Check if OK. Enter note number if deficient.

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Item | **GC** | **PC** | **EC** | **BC** | **CC** | **OR** | **A/E** | **CA** |
| Product documentation submitted |  |  |  |  |  |  |  |  |
| Related equipment Prefunctional Checklists completed |  |  |  |  |  |  |  |  |

# FUNCTIONAL PERFORMANCE VERIFICATIONS

**Demonstrate operation of equipment per contract documents including the following:**

Check if OK. Enter Outstanding Item Note number if deficient.

| **No** | **Item** | **GC** | **PC** | **EC** | **BC** | **CC** | **OR** | **A/E** | **CA** |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | Overhead Coiling |
|  |  |  |  |  |  |  |  |  |  |
| 1 |  Slide locking bolts engage through slots in tracks for locking by padlock on both the left and right jamb sides |  |  |  |  |  |  |  |  |
|  |   |  |  |  |  |  |  |  |  |
| 2 |  Chain-Hoist Operator for combination insulated service door and ventilation door operates smoothly throughout the door the range of the doors movement |  |  |  |  |  |  |  |  |
|  |   |  |  |  |  |  |  |  |  |
| 3 | Push-up Operation for Non-insulated Service Doors and Counter Doors – counterbalance mechanism allows the door to be lifted or pulled without exceeding 25lbf |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
| 4 | Door opens and closes without twisting or distortion |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
| 5 | A weather tight seal is maintained throughout the doors operation |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
| 6 | All hardware and operations assemblies operate smoothly and without making excessive noise |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |

# OUTSTANDING ITEMS

Note outstanding items in table below. Use numbers referenced above.

|  |  |  |
| --- | --- | --- |
| Resolved(Initial / Date) | **Note** | Description |
|  | **1.** |  |
|  | **2.** |  |
|  | **3.** |  |
|  | **4.** |  |
|  | **5.** |  |
|  | **6.** |  |
|  | **7.** |  |
|  | **8.** |  |
|  | **9.** |  |
|  | **10.** |  |

# FIELD NOTES

Fill in as appropriate.

|  |
| --- |
|  |
|  |
|  |
|  |
|  |

# SIGN OFF

System / Equipment has been installed in accordance with the Contract Documents and is ready for Owner acceptance.

|  |  |  |
| --- | --- | --- |
|  | **Signature** | **Date** |
| **Contractor’s Representative** |  |  |
| **A /E Representative** |  |  |
| **Commissioning Agent** |  |  |
| **Owner’s Representative** |  |  |

## END OF TEST